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How to make VG series 0.5 scroll pattern
                                                                       Astrodesign,Inc.      

 July 25, 2008
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1) Making 3840 x 1080 image (eg; If user has 1920 x 1080 image, required to convert it to double size by some consumer software, etc..).
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2)Dividing this 3840 x 1080 image to two images of “even” and “odd” lines below : 

  Save the image A) and B) in PC.
           1920                1920
      
                                            1080 
           (1111
      A)Even line only     B)Odd line only
3) Execute SP-8848 or SP-8870 first, then Image Converter ( Image Combine Form.  
<1> Check 0.5 pixel. 
 <2> Load A) Odd data on below 1, load B) Even data on below 2.

  <3> By pressing “Combine” key, 0.5 scroll data will be completed. 
  <4> Close by pressing Close key.
                 SP-8870                         SP-8848  

4) Execute 0.5 scroll pattern on VG(eg; refer to page 224 for VG-859C Ver.2.0 manual for its operation). 
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